### ISO 15415 Verification Tool Advanced Parameters

See the ISO 15415 Verification Tool Parameters section for details.

- ROI: Set the start point coordinates (x, y), width, height, and tilt angle of the region of interest (ROI).

- Auto Aperture size: When Auto Aperture is selected, sets the user-defined percentage of the decoded cell size. The aperture size will be set automatically based on the symbol's cell size.

- Dimension Units: When Auto Aperture is de-selected, allows you to enter units in mil or mm.

- Aperture Size: When Auto Aperture is de-selected, enter the Aperture value manually.

- Lighting Wave Length: Specifies the wavelength of the lighting being used. This value is for reporting only and does not affect verification results.

- Lighting Angle: Specifies the angle of the lighting being used. Note that this value is for reporting only and does not affect verification results.

- Setup Notes: Allws you to record any additional information that needs to be considered about your camera or lighting configuration.

Precautions for Correct Use: The ISO verification standards each provide a recommended or reference geometric, optical, and lighting configuration. You are encouraged to consult the latest revision of the standard to ensure compatibility. In broad terms, the goals of the standards are to specify measurement configurations that are consistent with appropriate or likely reading scenarios. If you deviate from the reference, you should include the light type, wavelength, and light configuration in the Setup Notes. The notes will be provided as part of the report.