### Point to Line Measure Tool Advanced Parameters

See the Point to Line Measure Tool Parameters section for details.

- ROI: Set the start point coordinates (x, y), width, height, and tilt angle of the region of interest (ROI).

- Input Point: Assign output points for any tool.

- Input Line: Assign output line for any tool.

- Lower/Upper Tolerance: Set lower and upper tolerance. (Range: 0 to 100,000)