### Point to Point Measure Tool Parameters

These parameters allow you to connect the two input points to output points from any other tool. The standard tolerance editor is also provided to allow the setting of an upper and lower measurement limit:

##### Input Point 1/2

- Input Point 1/2: Assign output points for any tool.

##### Distance Tolerance

- Lower/Upper Tolerance: Set lower and upper tolerance. (Range: 0 to 100,000)

##### Calibrate

See the Measurement Calibration section for details.