### Point to Line Measure Tool Parameters

These parameters allow you to connect the input point and line to an output point and line from any other tool. The standard tolerance editor is also provided to allow the setting of an upper and lower measurement limit:

##### Input Point

- Input Point: Assign output point for any tool.

##### Input Line

- Input Point: Assign output line for any tool.

##### Distance Tolerance

- Lower/Upper Tolerance: Set lower and upper tolerance. (Range: 0 to 100,000)

##### Calibrate

See the Measurement Calibration section for details.