### Select a device and Modify Device Settings

AutoVISION's Connect view allows you to select your device and configure its settings, and to create a new job.

The software emulator allows you to work from saved images without hardware.

Once a device is selected and its settings are configured, you can Create a New Job, Load a Job from a saved .avp file on your PC, or Upload Current Job from Device (your camera).

- Job: A completed program, including image acquisition, tools, and reporting.

- Tool: A self-contained set of steps used to perform a specific task.

Note: When operating in Emulator mode, there is no Upload Current Job from Device option.

Precautions for Correct Use: AutoVISION is not able to edit jobs that have been manipulated in FrontRunner. Switching jobs between AutoVISION and FrontRunner is not recommended.

##### Modifying Device Settings

When you click the Modify button, device settings under Details can be changed.

Note: If DHCP is disabled at startup and you click DHCP Enable, the IP Address and Subnet Mask fields are read-only and show the camera's current static IP Address and Subnet. If DHCP is enabled at startup, the IP Address and Subnet Mask assigned by DHCP are shown.

Precautions for Correct Use: The HAWK MV-4000 and the F4X0-F have different default IP addresses:

- The HAWK MV-4000’s default IP address is: 192.168.AA.BB, where AA.BB are the last 2 octets in decimal of the device MAC with subnet Class B 255.255.0.0. Set your PC to the same subnet (192.168.0.1, for example).

- The F4X0-F’s default IP address is: 192.168.188.2. Set the PC to same IP range (192.168.188.100, for example).