### Setting Up the ISO15415 Verification Tool

The flow of basic setting operation of the Symbol Quality Verification Tool is as follows.

1. Add a Symbol Quality Verification Tool to the image area.

2. Select the verification standard to use.

3. Adjust the search ROI to cover the area where you expect the symbol to be verified to move.

4. After specifying the verification conditions, execute calibration.

Precautions for Correct Use: When switching between ISO 15415, AIM DPM/ISO 29158, and ISO 15416, the links between tool outputs and GDS tags are lost. This is because the underlying components that make up the Symbol Quality Verification Tool are completely removed and then recreated whenever you change the tool's capability.