### Point to Point Measure Tool Outputs

- Status: Status is set to 1 if the measured value is within the tolerance. It is set to 0 if the measured value is not within the tolerance.

- Distance: The distance between the two input points.

- Horizontal Distance: Delta X between the two input points.

- Vertical Distance: Delta Y between the two input points.

- Pt to Pt Line: The line that runs through the two input points.

- MidPt: The point that is midway between the two input points.

##### Setup Time Feedback

In Edit mode, the tool will display the status and distance and it allows you to link outputs to tags within the software's Global Data Service (GDS). Refer to Link Menus for details.

In the image, an ‘X’ will be drawn everywhere an input edge point is found, and the straight line connected between two input edge points will also be drawn: