### ISO 15416 Verification Tool Outputs

- Status: True/False status of the tool.

##### Setup Time Feedback

In Edit mode, the tool will display the status of tool and Report Grade and it allows you to link outputs to tags within the software's Global Data Service (GDS). Refer to Link Menus for details.

Click on the letter grade in the tool list to open the verification report.

The report that is produced by AIM DPM/ISO 29158, ISO 15415, and ISO 15416 Symbol Quality Verification can be saved in either PDF or plain text format. Please see the Symbol Quality Verification Report for details.

##### ISO 15416 Verification Final Grade

The ISO 15416 final symbol grade is shown in the upper left corner and lower right corner of the verification report and the numeric grade is reported as the first field in the reported grade string. The ISO 15416 final symbol grade is a compilation of the 10 individual scan line final grades applied over the region of the symbol. Each individual scan grade from the 10 scans applied can be found at the bottom of each scan column. This scan grade is the lowest grade from that individual scan. The final symbol grade is the average result of the 10 individual scans. In the follow example you see scans 1-5 have quiet zone violations and receive a grade of F or grade value 0. The scans 6-10 receive a B grade based on the minimum grade of modulation. The final symbol grade is the average of the final scans (0 + 0 + 0 + 0 + 0 + 3 + 3 + 3 + 3 + 3) / 10 = 1.5 or grade C. Note that if custom verification is enabled individual parameters can be removed from the scan grade and final grade calculation.

##### ISO 15416 Numeric Score and Grade Level Comparison

##### Verification Results

All verification output values can be output through Inspection Outputs. All verification status outputs can be tied to the camera's Digital Outputs.