### Step 5 – Start Calibration and Check Results

Now that the camera and target are set up correctly and the calibration dots are being counted correctly, it is time to run the calibration.

Click the Run Calibration button and the utility will process the data from the image and generate the calibration matrices. The utility will provide feedback in the Calibration Status area as shown in the image below.

The data output includes pass / fail status and, if successful, the approximate conversion from pixels to the user-defined real-world units along with the focus setting the camera used.

The graphics in the image will change to show the grid of calibration points with the origin point marked in green (a custom origin point of 3,5 was defined in Step 3) and the axis orientation indicated in the top-left of the buffer.

Proceed to the final step.