### Report Gasket Inspection Status and Gasket Height

Click on Inspection Outputs in the job list to report inspection status and gasket height. Set the following output parameters:

- Use TCP/Serial Output for Emulator testing.
- Add formatting around inspection status and measurement value.

- Telnet to 127.0.0.1 to check the data format.

Note: See TCP/Serial Output for a description of how to use Telnet to view TCP output.