### Step 6 – Save Calibration File to Disk or Camera

The calibration data generated by the utility must now be saved to disk so that it can be used in AutoVISION. Click the Save Calibration… button and choose a file name. The utility will default to the Vscape/Jobs/Calib. This is the recommended directory.

Click Save Calibration.

Once the calibration is saved, click Finish (or Exit) to leave the utility.