### Lighting Option

Allows you to select between Off, On, Strobe, Power Strobe, or External Strobe. Power Strobe mode is limited to a maximum 1 ms pulse width (as with Omron Microscan's NERLITE Smart Series Illuminators).

When Lighting is set to Off, external lighting is disabled, and internal lighting is turned off.

When Lighting is set to On, external lighting is enabled (Output 3 is placed in a de-energized or open state) and internal lighting is enabled.

When Lighting is set to Strobe, Output 3 is enabled to control an external light. The normal state for Output 3 in this configuration is in an energized or closed state. At the start of an image acquisition the output is de-energized or placed in an open state. At the end of the camera's exposure period, the output is set back to a closed state. Strobe operation allows you to connect the appropriate NERLITE external lighting product for your application and to control that light in sync with image acquisition. The light can be switched on fast enough that it is at full brightness before the exposure begins.

##### Power Strobe and External Strobe

Power Strobe and External Strobe allow you to select different lighting configurations when acquiring an image.

Precautions for Correct Use: Power Strobe does not function with rolling shutter.

##### Lighting Select

Allows you to select between Internal WHT, Internal RED, or Expansion lighting. This setting is used in conjunction with the Lighting Mode selection.

##### External Strobe Control

Allows you to select which output is used to control the External Strobe. The selected output is no longer available for use elsewhere in the job.

##### Lighting Mode Table