## Quick Start

There are six basic steps required to set up a camera with AutoVISION:

- Configure hardware. Set up the camera, cabling, power supply, and I/O.

- Select a device and create a new job. Use the Connect view to select a device and create a new job or load an existing job.

- Adjust camera settings. Use the Connect and Image views to adjust parameters specific to the connected smart camera.

- Edit the job. Add and configure AutoVISION tools that are useful for your application. Use Inspection Outputs parameters to configure job outputs.

- Run the job. Jobs are downloaded to the camera when entering the Run view, but are not saved yet.

- Save the job. Stop the job and click the Save icon to save the current job on the camera, but don’t forget to start the job again.