### ISO 15415 Verification Tool Outputs

##### ISO 15415 Verification Report

- Status: True/False status of the tool.

##### Setup Time Feedback

In Edit mode, the tool will display the status of tool and Report Grade and it allows you to link outputs to tags within the software's Global Data Service (GDS). Refer to Link Menus for details.

Click on the letter grade in the tool list to open the verification report.

The report that is produced by AIM DPM/ISO 29158, ISO 15415, and ISO 15416 Symbol Quality Verification can be saved in either PDF or plain text format. Please see the Symbol Quality Verification Report for details.

##### ISO 15415 Verification Final Grade

The ISO 15415 final grade is shown in the upper left corner of the verification report and the numeric value is reported as the first field in the reported grade string. The final grade is defined by the lowest grade achieved by any individual grade parameter.

When custom verification is enabled, in addition to setting threshold for Good/Fair/Poor, you have the option to select which parameters are to be included in the final grade calculation. In the below example you can see the impact of removing Axial Non-Uniformity from the grade calculation.

##### ISO 15415 Numeric Score and Grade Level Comparison

##### Verification Results

All verification output values can be output through Inspection Outputs. All verification status outputs can be tied to the camera's Digital Outputs.