### Inspection Statistics

The Run view provides the following statistics:

- Tool Results: Shows the Pass/Fail status and inspection data from each of your tools.

- Inspection Counts: Displays the number of parts inspected, passed and rejected.

- Inspection Timing Statistics: Displays statistics on the speed of your inspection.

1. Process: The amount of time spent running all the tools. It does not count the time to take the picture;

   1. Draw: The amount of time spent drawing the screen graphics;

   2. Cycle: When triggered, this is the total time between the current trigger and the previous one. When free-running, it is the time between the current image acquire and the previous one.

   3. Cycle Worst: The longest Cycle Time since the start of the job.

   4. PPM: The parts-per-minute rate for the inspection.

   5. PPM Worst: The lowest parts-per-minute rate for the inspection since the start of the job.

   6. Overruns: Shows if inspection is being triggered faster than inspections can be performed.