## Firmware Updates

AutoVISION’s simple Device Firmware Update feature makes it easy to download and install firmware on your camera.

To download and install firmware:

- Navigate to Device Firmware Update.

- After you click Device Firmware Update, the Smart Camera Firmware Update Tool will appear. Select your camera from the Please Select a Smart Camera to Update dropdown menu.

  Precautions for Correct Use: Only cameras on the same network as your PC will be visible in this menu.

- Once you have selected your camera, its identifying details, such as Model, Firmware Version, MAC Address, IP Address, Status, and PC Version will be displayed.

- Select the desired version of firmware from the Select the Firmware Version dropdown menu. This menu will list all the firmware versions on your PC.

  Note: The firmware versions shown below are representative examples and may not necessarily reflect what you see on the dropdown menu.

- Click the Update Firmware button.

- A dialog will appear asking Are you sure you wish to update this camera? Click Yes.

- If a username and password have been defined for the camera, a second dialog will then appear prompting you for your username and password.

  Precautions for Correct Use: The user name and password are both case-sensitive. Click OK after you have entered your user name and password to begin the download and install process.

The firmware update process may take more than a minute.

Once the firmware is downloaded and installed, the camera will reboot.

- When the entire firmware update process is complete, click the Exit button to close the utility.

Precautions for Correct Use: The camera’s firmware version must match the version of software being used to run jobs on the PC. If the firmware update fails, repeat the process. If it fails a second time, please contact OMRON technical support.